

CONVENTIONAL TIMBER VS BALANCE ORDER FORM

**PLEASE SEND TO CALDWELL HARDWARE VIA EMAIL: SALES@CALDWELL.CO.UK OR FAX: 024 7643 7969**

CUSTOMER DETAILS Order No.

      Contact:

      Delivery Date:

      Tel. No.

      Fax No.

Balances housed in Outer Frame  OR Balances housed in Sash

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Georgian Bars (Plant on type)**  **(If Yes- Specify no. Horizontal & no. Vertical Bars)** | YES |  | NO |  |
| HORIZONTAL |  | VERTICAL |  |
| **Pre-tensioned balances only** | YES |  | NO |  |
| **Torso balances only** | YES |  | NO |  |
| **Wood Type** | Softwood |  | Hardwood |  |

**THIS ORDER FORM MUST ONLY BE USED WHEN ORDERING SASH BALANCES**

FOR USE WITH CONVENTIONAL TIMBER VERTICAL SLIDING WINDOWS

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Ref. | QUANTITY OF WINDOWS | DIM “W” (mm) | DIM “A” (mm) | DIM “B” (mm) | DIM “C” (mm) | DIM “D” (mm) | SIZE OF HORN | GEORGIAN BARS  (Tick) | GLAZING CONFIG.  E.G. 6-12-6 | GLAZED SASH  WEIGHT (kg) | |
|  |  |  |  |  |  |  |  |  |  |  | UPPER |
|  | LOWER |
|  |  |  |  |  |  |  |  |  |  |  | UPPER |
|  | LOWER |
|  |  |  |  |  |  |  |  |  |  |  | UPPER |
|  | LOWER |
|  |  |  |  |  |  |  |  |  |  |  | UPPER |
|  | LOWER |
|  |  |  |  |  |  |  |  |  |  |  | UPPER |
|  | LOWER |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| White Tubes |  | White travel Stops |  | Brown Tubes |  | Brown Travel Stops |  |


|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | Qty |  | Qty |  | Qty |  | Qty |
| **Side Fix Brackets** | UK121 |  | UK120 |  | UK212 |  | UK835 |  |
| **Bottom Fix Brackets** | UK136 |  | UK632 |  | WS60-32 |  |  |  |
| **Nyclad Brackets** | WDST75-47 |  | UK115N |  | UK114N |  | UK101N |  |

**NOTE:** Sash weights are based on 50mm square profile in softwood unless otherwise stated.

For accuracy it is preferable that you provide a fully glazed sash weight.

We cannot accept responsibility for goods supplied incorrectly if accurate sash weights have not been provided.

### WINDOW DETAILS



**PLEASE REQUEST DATA SHEET 00363 FOR WINDOW DIMENSION TERMINOLOGY**

|  |
| --- |
| **THIS ORDER IS ACCEPTED UNDER OUR CURRENT ‘TERMS & CONDITIONS OF SALE’ COPIES AVAILABLE UPON REQUEST.** |